**How do you clean the Passy-Muir Valve?**

**1.** **Swish Valve daily in soapy, warm water (not hot water)**.

**2.** **Rinse Valve very thoroughly in warm running water.**

**3.** **Allow Valve to air dry thoroughly** before placing in storage container. Do not apply heat to dry Valve.

**4.** DO NOT use hot water, peroxide, bleach, vinegar, alcohol, brushes or cotton swabs to clean Valve.

**Remember with your Valve:**

**-** Don’t wear it while sleeping or even napping

- Take the valve off before you cough

-If you cough and phlegm or blood gets in the valve need to clean it before wearing again

-If the valve starts to make funny noises first: make sure it is clean, if cleaning doesn’t fix the problem it may be time to replace it